HVAC Components. Chevrolet Metro 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Clutch | Right side of engine compartment, front of A/C compressor | -- | --
A/C Compressor Control Module | Below right side of the IP, attached to evaporator case | HVAC Component Views | HVAC Connector End Views
A/C Condenser Fan Motor | Right side of grille, front of A/C condenser | HVAC Component Views | --
A/C Refrigerant (Dual) Pressure Switch | Right rear side of the engine compartment, near the strut tower | -- | --
A/C Switch | Center of IP, above radio | -- | HVAC Connector End Views
Blower Motor | Behind the right side of the IP | Heater Blower Controls Component Views | Heater Blower Controls Connector End Views
Blower Motor Resistor | Behind the right side of the IP, in blower assembly | Heater Blower Controls Component Views | Heater Blower Controls Connector End Views
Blower Speed Selector Switch | Center of IP, above radio | Heater Blower Controls Component Views | --
Fuse Box | Left side of the engine compartment, mounted on Left inner side of the fender, behind the relay box | Power and Grounding Component Views | Power and Grounding Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Relay Box | Left front engine compartment, near the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
C111 (2 Cavities) (With A/C) | Main harness to A/C jumper harness, right rear side engine compartment below front wiper motor | Harness Routing Views | --
C112 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near bulkhead | Harness Routing Views | Inline Harness Connector End Views
C113 (16 Cavities) | Main harness to engine harness, right rear side of the engine compartment near the bulkhead | Harness Routing Views | Inline Harness Connector End Views
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C208 (8 Cavities) | Main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
C211 (6 Cavities) | IP harness to blower speed selector switch jumper, behind the center of the IP | Harness Routing Views | --
G102 | Left front side of the engine compartment on the left front inner fender near battery | Harness Routing Views | --
G103 | Right front side of the engine compartment on the right front side of the inner fender | Harness Routing Views | --
G201 | Behind the left side of the kick panel | Harness Routing Views | --
G202 | Right side of the center IP behind the radio | Harness Routing Views | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
P202 | Center of the engine compartment, on the bulkhead | Harness Routing Views | --
S122 | Main harness, at relay box | Harness Routing Views | --
S123 | Main harness, approximately 4 cm (2 in) from brake fluid level switch connector breakout | Harness Routing Views | --
S134 | A/C jumper harness, approximately 15 cm (6 in) from the G103 breakout | -- | --
S202 | Main harness, approximately 8 cm (3.125 in) from the junction block connector C6 breakout | -- | --
S207 | Main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S209 | Main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S210 | Main harness, approximately 15 cm (6 in) from C208 | -- | --
S213 | Main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S232 | IP harness, approximately 4 cm (2 in) from the C205 breakout | Harness Routing Views | --
S233 | IP harness, approximately 8 cm (3.125 in) from the blower motor branch breakout | Harness Routing Views | --
S234 | IP harness, approximately 1 cm (.375 in) from the diode module connector breakout | Harness Routing Views | --
S238 | IP harness, approximately 3 cm (1.19 in) from the blower motor connector breakout | Harness Routing Views | --
S243 | IP harness, approximately 5 cm (2 in) from the cigar lighter connector breakout | Harness Routing Views | --
S247 | Main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S254 | IP harness, approximately 6 cm (2.375 in) from the C215 breakout | Harness Routing Views | --