Rear Door Jamb Switch Replacement. Chevrolet Metro 2000

For 1990-2009 cars

### Removal Procedure

1. Open the rear side door.
2. Open the rubber cap in order to gain access to the door-jamb switch screw.
3. Remove the screw that retains the door-jamb switch to the door jamb.
4. Disconnect the door jamb switch electrical connector.
5. Remove the door-jamb switch from the vehicle.

### Installation Procedure

1. Connect the door jamb switch electrical connector.
2. Install the door-jamb switch to the door jamb. Secure the switch with the screw.
3. Close the rubber cap.
4. Close the rear side door.