Washers Inoperative. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Turn the ignition switch to the ON position.
2. Backprobe the front washer pump connector with a test lamp from cavity 1 to ground.
3. Pull the front wiper/washer switch lever.

Does the test lamp light?

--

Go to Step 4

Go to Step 3

3 | Test for an open in the BLU/BLK wire between the combination switch and the front washer pump. Was an open found? | -- | Go to Step 5 | Go to Step 6
4 | Test for an open in the BLK wire between the front washer pump and G102. Was an open found? | -- | Go to Step 5 | Go to Step 7
5 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
7 | Replace the front washer pump. Refer to Washer Pump Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --