Engine Coolant Temperature Gage Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster from the instrument panel. Refer to Instrument Cluster Replacement .
2. Push on the tabs in order to remove the cluster lens (7) and the bezel assembly (6) from the cluster housing.
3. Remove the 3 screws (4) that secure the temperature gauge to the cluster housing.
4. Remove the temperature gauge (4) from the cluster housing (3).

### Installation Procedure

1. Install the temperature gauge (4) to the cluster housing (3).
2. Secure the temperature gauge to the cluster housing with 3 screws (4).
3. Install the cluster lens (7) and the bezel (6) to the cluster housing.
4. Install the instrument cluster to the instrument panel. Refer to Instrument Cluster Replacement .