Front License Plate Bracket Replacement. Chevrolet Metro 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws (8) that retain the license plate.
2. Remove the license plate (7).
3. Remove the 2 screws (5) that retain the front license plate bracket.
4. Remove the front license plate bracket (4) from the front bumper fascia (2).

### Installation Procedure

1. If you are installing the front license plate bracket (4) for the first time, perform the following steps:

1.1. | Drill a pilot hole at each dimple (1) in the front bumper fascia (2).The diameter should be 4 mm (5/32 in), and the depth should be approximately 3 mm (1/8 in).

1.2. | Enlarge the pilot holes to approximately 8 mm (5/16 in) and to approximately 3 mm (1/8 in) deep.

2. Install 2 spring nuts (6) to the front license plate bracket (4) in the following circumstances:

2.1. | You are installing the bracket for the first time.

2.2. | The spring nuts (6) are missing

3. Install the bracket (4) to the front bumper fascia (2). Secure the bracket with the 2 screws (5).
4. Install the license plate (7) to the bracket (4). Secure the license plate with the 2 screws (8).