Wipers Always On. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Disconnect the junction block connector C6.
2. Turn the ignition switch to the ON position.

Do the wipers stop?

--

Go to Step 4

Go to Step 3

3 | Test for a short to voltage in the BLU wire or the BLU/RED wire between the combination switch and the front wiper motor. Was a short to voltage found? | -- | Go to Step 5 | Go to Step 6
4 | Replace the front wiper motor. Refer to Windshield Wiper Motor Replacement . Is the repair complete? | -- | Go to Wiper/Washer System Check | --
5 | Repair the short. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in SIR. Is the repair complete? | -- | Go to Wiper/Washer System Check | --