Power Door Systems Components. Chevrolet Metro 2001

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in Wiring Systems | Power and Grounding Connector End Views in Wiring Systems
LH Front Power Door Lock Actuator (4-Door With Power Door Locks) | The left front door on the door-latch assembly | Power Door Systems Component Views | Power Door Systems Connector End Views
LH Power Door Lock Switch (4-Door With Power Door Locks) | The trim panel on the left front door | Power Door Systems Component Views | Power Door Systems Connector End Views
LH Rear Power Door Lock Actuator (4-Door with Power Door Locks) | The left rear door, on the door-latch assembly | Power Door Systems Component Views | Power Door Systems Connector End Views
Power Door Lock Control Module (4-Door with Power Door Locks) | The left side of the IP, mounted to the A-pillar, above the left kick panel | Power Door Systems Component Views | Power Door Systems Connector End Views
RH Front Power Door Lock Actuator (4-Door with Power Door Locks) | The right front door, on the door-latch assembly | Power Door Systems Component Views | Power Door Systems Connector End Views
RH Power Door Lock Switch (4-Door With Power Door Locks) | In the trim panel of the right front door | Power Door Systems Component Views | Power Door Systems Connector End Views
RH Rear Power Door Lock Actuator (4-Door with Power Door Locks) | The right rear door, on the door-latch assembly | Power Door Systems Component Views | --
C212 (6 Cavities) (4-Door) | The floor harness to the left front door, behind the left kick panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C213 (6 Cavities) (4-Door) | The floor harness to the right front door, behind the right kick panel | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C306 (2 Cavities) (4-Door With Power Door Locks) | The floor harness to the left rear door harness, which is attached to the left side B-pillar | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
C307 (2 Cavities) (4-Door With Power Door Locks) | The floor harness to the right rear door harness, which is attached to the right side B-pillar | Harness Routing Views in Wiring Systems | Inline Harness Connector End Views in Wiring Systems
G203 | The junction-block case ground, under the left side of the IP | -- | --
P304 (4-Door With Power Door Locks) | The right rear door jamb | -- | --
P500 | The left front door | -- | --
P600 | The right front door | -- | --
P700 (4-Door With Power Door Locks) | The left rear Door | -- | --
P800 (4-Door With Power Door Locks) | The right rear door | -- | --
S307 (4-Door With Power Door Locks) | The floor harness, which is approximately 5 cm (2 in) from the control-module connector breakout for the power door lock | Harness Routing Views in Wiring Systems | --
S308 (4-Door With Power Door Locks) | The floor harness, which is approximately 10 cm (4 in) from the control-module connector breakout of the power door lock | Harness Routing Views in Wiring Systems | --
S314 (4-Door With Power Door Locks) | The floor harness, which is approximately 25 cm (10 in) from the C201 breakout | Harness Routing Views in Wiring Systems | --