Cylinder Head Disassemble. Chevrolet Metro 2001

For 1990-2009 cars

#### Tools Required

• | J 8062 Valve Spring Compressor

• | J 37979 Valve Spring Compressor Adaptor

• | J 36017 Valve Guide Seal Remover

Important: Keep the valve train components together, and identify the components so that you can correctly install the components in the original position.

Caution: Wear safety glasses in order to avoid eye damage.

1. Compress the valve spring. Use the J 8062 .
2. Remove the valve keepers.
3. Slowly release the J 8062 from the valve spring assembly.
4. Remove the retainer (1).
5. Remove the spring.

Notice: Do not damage the valve guide. Remove any burrs that have formed at the key groove by chamfering the valve stem with an oil stone or a file.

6. Remove the valve seal. Use the J 36017 .
7. Remove the spring seats.
8. Remove the valve.
9. Remove the remaining valves.