Temperature Control Cable Replacement. Chevrolet Metro 1998

For 1990-2009 cars

### Removal Procedure

Important: Note the routing of the cable to make installation easier.

1. Disconnect the temperature control cable (6) at the heater case (1).
2. Remove the heater control unit (5). Refer to Control Assembly Replacement .
3. Disconnect the temperature control cable at the heater control unit.
4. Remove the temperature control cable from the instrument panel (IP).

### Installation Procedure

1. Position the temperature control cable (6) in the vehicle. Route the cable as previously noted.
2. Connect the temperature control cable to the heater control unit.
3. Install the heater control unit (5). Refer to Control Assembly Replacement .
4. Connect the temperature control cable to the heater case (1).
5. Adjust the temperature control cable. Refer to Temperature Control Cable Adjustment .