Body Waterleak Repair. Chevrolet Metro 1999

For 1990-2009 cars

In order to locate the exact leak point, or in order to repair the leak, you may have to remove some interior trim panels or some components. Refer to Recommended Materials (Waterleak Repair) .

After completion of any waterleak repair, retest the general area using the water-test stand. Do not use high pressure air or a water hose for testing repaired areas. The fresh repair material may disassemble under abnormal pressure.