Main Relay Replacement. Chevrolet Metro 1998

For 1990-2009 cars

### Removal Procedure

1. Disconnect the Negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.

2. Remove the relay box cover from the relay box.
3. Remove the main relay (1) from the relay box (2).

### Installation Procedure

1. Install the main relay (1) into the relay box (2).
2. Install the relay box cover to the relay box.
3. Connect the Negative battery cable. Refer to

   Caution: Unless directed otherwise, the ignition and start switch must be in the OFF or LOCK position, and all electrical loads must be OFF before servicing any electrical component. Disconnect the negative battery cable to prevent an electrical spark should a tool or equipment come in contact with an exposed electrical terminal. Failure to follow these precautions may result in personal injury and/or damage to the vehicle or its components.