Parking and Turn Signal Lamp Bulb Replacement. Chevrolet Metro 2000

For 1990-2009 cars

### Removal Procedure

1. Remove the 2 screws (1, 7) that retain the headlamp (6).
2. Turn the socket of the park and turn lamp bulb (8) counterclockwise in order to remove the socket from the headlamp (6).
3. Remove the park and turn lamp bulb (8) from the socket.

### Installation Procedure

1. Install the park and turn lamp bulb (8) to the socket.
2. Rotate the socket of the park and turn lamp bulb (8) clockwise in order to secure the socket to the headlamp (6).
3. Install the headlamp (6) to the vehicle. Secure the headlamp with the 2 screws (1, 7).
4. Adjust the headlamp aim. Refer to Headlamp Aiming .