Dome Lamps Inoperative. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Values | Yes | No
--- | --- | --- | --- | ---
1 | Was the Interior Lights System Check performed? | -- | Go to Step 2 | Go to Interior Lamps System Check
2 | Backprobe the dome lamp connector with a test lamp from cavity 2 to ground. Does the test lamp light? | -- | Go to Step 3 | Go to Step 4
3 | Replace the dome lamp assembly. Refer to Dome Lamp Replacement . Is the repair complete? | -- | Go to Interior Lamps System Check | --
4 | Test for an open in the WHT wire between the junction block and the dome lamp. Was an open found? | -- | Go to Step 5 | Go to Step 6
5 | Replace the junction block. Is the repair complete? | -- | Go to Interior Lamps System Check | --
6 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Interior Lamps System Check | --