Defogger System Check. Chevrolet Metro 2001

For 1990-2009 cars

Step | Action | Normal Results | Abnormal Result(s)*
--- | --- | --- | ---

1

1. Turn the ignition switch to the ON position.
2. Press the rear defogger switch to the ON position.

The rear defogger indicators light, and the rear windows warm up.

• | Defogger Lamp Switch Inoperative - Rear Window

• | Defogger Inoperative - Rear Window, Indicator Lamp On

* Refer to the appropriate symptom diagnostic table for the applicable abnormal result.