Camshaft Removal. Chevrolet Metro 1998

For 1990-2009 cars

1. Remove the camshaft timing belt pulley.
2. Remove the outboard ignition coil from the camshaft sensor housing.
3. Remove the camshaft sensor from the camshaft sensor housing.
4. Remove the three camshaft sensor housing bolts (2) and the camshaft sensor housing from the cylinder head.

Important: In order to catch any oil, place a shop rag under the camshaft housing before removing it from the cylinder head.

5. Loosen all valve adjusting screw lock nuts (2), turn adjusting screws back all the way to allow all rocker arms to move freely.
6. Gradually remove the twelve camshaft housing bolts in the sequence shown.
7. Remove the camshaft.