Front Side Door Inside Handle Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Pull the water deflector far enough away from the door in order to gain access to the inside door handle (5).
3. Remove the 2 screws and the inside door handle (5) from the door.
4. Remove the following components from the inside door handle (5):

• | The handle rod

• | The handle lock rod

### Installation Procedure

1. Install the following components to the inside door handle (5):

• | The handle rod

• | The handle lock rod

2. Install the inside door handle (5) to the door. Secure the handle with the 2 screws.
3. Apply adhesive to the back of the water deflector.
4. Place the water deflector in a normal position.
5. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement .