Instrument Panel Outer Air Outlet Deflector Replacement - Left Side. Chevrolet Metro 1998

For 1990-2009 cars

### Removal Procedure

1. Gently pry-out the left vent garnish (5) with a small flat screwdriver from the IP.
2. Remove the IP center outlet duct. Refer to Instrument Panel Air Outlet Ducts Replacement in Heating, Ventilation and Air Conditioning or Instrument Panel Air Outlet Ducts Replacement in HVAC Systems - Manual.
3. Remove the 2 screws and the left vent louver (6) from the IP.

### Installation Procedure

1. Install the left vent louver (6) to the IP. Secure the louver with the 2 screws.
2. Install the left vent garnish panel (5) to the IP. Push the panel in until the panel fully engages.
3. Install the IP center outlet duct. Refer to Instrument Panel Air Outlet Ducts Replacement in Heating, Ventilation and Air Conditioning or Instrument Panel Air Outlet Ducts Replacement in HVAC Systems - Manual.