Power and Grounding Components. Chevrolet Metro 2001

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Control Module | Below the right side of the IP, attached to the evaporator case | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
A/C Condenser Fan Motor | The right side of the grille, in front of the A/C condenser | HVAC Component Views in HVAC | --
A/C Refrigerant (Dual) Pressure Switch | The right rear side of the engine compartment, near the strut tower | -- | --
A/C Switch | The center of the IP, above the radio | -- | HVAC Connector End Views in HVAC
Audio Alarm Module | The left side of the lower IP, to the left of the steering column | Audible Warnings Component Views in Instrument Panel, Gauges and Console | Audible Warnings Connector End Views in Instrument Panel, Gauges and Console
Backup Lamp Switch (Manual Transaxle) | The left side of the engine compartment, the top of the transaxle | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Battery | The left side of the engine compartment | Power and Grounding Component Views | --
Blower Motor | Behind the right side of the IP | HVAC Component Views in HVAC | HVAC Connector End Views in HVAC
Blower Speed Selector Switch | The center of the IP, above the radio | HVAC Component Views in HVAC | --
Brake Fluid Level Switch | In the brake-fluid reservoir | -- | Hydraulic Brake Connector End Views
Camshaft Position Sensor (VIN 2) | The cylinder head, near the ignition coil 2 | Engine Controls Component Views in Engine Controls | --
Center High-Mounted Stoplamp (CHMSL) | The bottom of the rear window | -- | Lighting Systems Connector End Views in Lighting Systems
Cigar Lighter | The center of the IP, below the radio | -- | Power and Grounding Connector End Views
Clutch Pedal Position (CPP) Switch (Manual Transaxle) | Mounted above the clutch pedal | Engine Electrical Component Views in Engine Electrical | --
Data Link Connector (DLC) OBD 2 | Below the left side of the IP, near the center console | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Daytime Running Lamps (DRL) Control Module | Behind the left side of the IP | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Duty Check Data Link Connector | The passenger compartment, taped to the harness behind the IP compartment | Data Link Communications Component Views in Data Link Communications | Data Link Communications Connector End Views in Data Link Communications
Early Fuel Evaporation (EFE) Heater (VIN 6) | Mounted between the intake manifold and the throttle body | Engine Controls Component Views in Engine Controls | --
Electronic Brake Control Module (EBCM) (With ABS) | Behind the left IP, above the junction block | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
Engine Cooling Fan Motor | The left front side of the engine compartment, behind the radiator | -- | Cooling System Connector End Views in Engine Cooling
Front Washer Pump | The left front side of the engine compartment, under the washer fluid reservoir | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Front Wiper Motor | The right rear side of the engine compartment, against the bulkhead | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Fuel Sender Assembly | In the fuel tank | Engine Controls Component Views in Engine Controls | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Fuse Box | The left side of the engine compartment, mounted on the left inner side of the fender, behind the relay box | Power and Grounding Component Views | Power and Grounding Connector End Views
Generator | The right rear side of the engine compartment, mounted to the engine | Engine Electrical Component Views in Engine Electrical | --
Heated Oxygen Sensor 1 (HO2S1) | The front of the engine in the exhaust manifold | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Heated Oxygen Sensor 2 (HO2S2) | Below the vehicle after a three-way catalytic converter (TWC) | Engine Controls Component Views in Engine Controls | --
Horn | The left front side of the engine compartment, behind the grille | Horn Component Views in Horns | --
Idle Air Control (IAC) Valve (VIN 2) | The top of the engine, mounted to the throttle body | Engine Controls Component Views in Engine Controls | Engine Controls Connector End Views in Engine Controls
Idle Speed Control (ISC) Motor (VIN 6) | The top of the engine, mounted to the throttle body | Engine Controls Component Views in Engine Controls | --
Ignition Control Module (VIN 6) | The left engine compartment on the bulkhead near the strut tower | Engine Controls Component Views in Engine Controls | --
Ignition Coil (VIN 6) | The left side of the engine compartment, on the bulkhead | Engine Controls Component Views in Engine Controls | --
Ignition Coil 1 (VIN 2) | On the cylinder head, over spark plug 4 | Engine Controls Component Views in Engine Controls | --
Ignition Coil 2 (VIN 2) | On the cylinder head, over spark plug 2 | Engine Controls Component Views in Engine Controls | --
Ignition Key Warning Switch | The right side of the steering column, on the ignition-switch cylinder | -- | --
Ignition Switch | The right side of the steering column | -- | --
Illumination Controller | In the IP, to the left of the steering column | -- | Lighting Systems Connector End Views in Lighting Systems
Inflatable Restraint Forward Discriminating Sensor | The front center of the grille, behind the hood latch assembly | SIR Component Views in SIR | --
Inflatable Restraint Sensing and Diagnostic Module (SDM) | The center of the console, in front of the manual selector | SIR Component Views in SIR | SIR Connector End Views in SIR
Instrument Panel Cluster Assembly | The left side of the IP | -- | Instrument Panel, Gages, and Console Connector End Views in Instrument Panel, Gauges and Console
Junction Block | Behind the left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Lamp Driver Relay (With ABS) | Behind the left side of the IP, to the left of the steering column, near the electronic brake control module (EBCM) | Antilock Brake System Component Views in Antilock Brake System | Antilock Brake System Connector End Views in Antilock Brake System
LH Power Door Lock Switch (4-Door With Power Door Locks) | The trim panel of the left front door | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Luggage Compartment Lamp (4-Door) | The center of the luggage compartment, under the rear-window shelf | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Noise Suppressor Filter (VIN 6) | The left rear engine compartment, taped to the harness, below the ignition control module | Engine Controls Component Views in Engine Controls | --
Power Door Lock Control Module (4-Door with Power Door Locks) | The left side of the IP, mounted to the A-pillar, above the left kick panel | Power Door Systems Component Views in Doors | Power Door Systems Connector End Views in Doors
Powertrain Control Module (PCM) | Behind the right side of the IP, near the glove box | Engine Controls Component Views in Engine Controls | Powertrain Control Module Connector End Views in Engine Controls
Radio | Center of the IP | -- | Entertainment Connector End Views in Entertainment
Rear Defogger | In the rear window | Stationary Windows Component Views in Stationary Glass | --
Rear Defogger Switch | In the IP, to the left of the steering column | -- | Stationary Windows Connector End Views in Stationary Glass
Rear Washer Pump (2-Door LSi) | The left front side of the engine compartment under the washer fluid reservoir | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Rear Wiper Motor (2-Door LSi) | The center of the liftgate | Wiper/Washer Component Views in Wipers/Washer Systems | Wiper/Washer Connector End Views in Wipers/Washer Systems
Rear Wiper/Washer Switch (2-Door LSi) | In the IP, to the left of the steering column | -- | Wiper/Washer Connector End Views in Wipers/Washer Systems
Relay Box | The left front engine compartment, near the battery | Power and Grounding Component Views | Power and Grounding Connector End Views
RH Power Door Lock Switch (4-Door With Power Door Locks) | In the trim panel of the right front door | Power Door Systems Component Views | Power Door Systems Connector End Views
Seat Belt Switch | In the left seat belt buckle | -- | Audible Warnings Connector End Views in Antilock Brake Systems
Shift Lock Solenoid (Automatic Transaxle) | Near the base of the manual selector | -- | --
Starter Solenoid | The center rear of the engine, at the top of the starter motor | Engine Electrical Component Views in Engine Electrical | --
Stoplamp Switch | The top of the brake pedal | Lighting Systems Component Views in Lighting Systems | Lighting Systems Connector End Views in Lighting Systems
Supplemental Inflator Restraint Data Link Connector (SIR DLC) | Behind the left lP, near the junction block | -- | Data Link Communications Connector End Views in Data Link Communications
Transaxle Range Switch (Automatic Transaxle) | The left side of the engine compartment, mounted to the top of the transaxle | -- | Automatic Transmission Connector End Views in Automatic Transmission
Turn Signal/Combination Switch | On the steering column | -- | Lighting Systems Connector End Views in Lighting Systems
C112 (16 Cavities) | The main harness to the engine harness, on the right rear side of the engine compartment near the bulkhead | Harness Routing Views | Inline Harness Connector End Views
C113 (16 Cavities) | The main harness to the engine harness, on the right rear side of the engine compartment near the bulkhead | Harness Routing Views | Inline Harness Connector End Views
C200 (12 Cavities) | The main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
C204 (2 Cavities) (Manual Transaxle) | The main harness to the clutch pedal position switch, behind the left side of the IP | Harness Routing Views | --
C207 (3 Cavities) | The IP harness to the dome lamp harness, on the right side of the upper cowl | Harness Routing Views | Inline Harness Connector End Views
C208 (8 Cavities) | The main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
C210 (5 Cavities) | The supplemental inflatable restraint (SIR) harness to the IP harness, behind the left side of the IP, near the junction block | Harness Routing Views | Inline Harness Connector End Views
C211 (6 Cavities) | The IP harness to the selector switch jumper for the blower speed , behind the center of the IP | Harness Routing Views | --
C212 (6 Cavities) (4-Door) | The floor harness to the left front door, behind the left kick panel | Harness Routing Views | Inline Harness Connector End Views
C213 (6 Cavities) (4-Door) | The floor harness to the right front door, behind the right kick panel | Harness Routing Views | Inline Harness Connector End Views
C300 (2 Cavities) | The floor harness to the fuel tank jumper harness, under the rear passenger seat | Harness Routing Views | Inline Harness Connector End Views
C311 (3 Cavities) | The floor harness to the fuel tank jumper harness, under the rear passenger seat | Harness Routing Views | Inline Harness Connector End Views
C400 (10 Cavities) (4-Door) | The floor harness to the luggage-compartment harness, on the left front side of the luggage compartment near the left-rear speaker | Harness Routing Views | --
C402 (6 Cavities) (2-Door) | The floor harness to the liftgate harness, at the right rear corner of the vehicle | Harness Routing Views | --
G100 | Mounted on top of the left side of the transaxle | -- | --
G101 | The left front side of the engine compartment, in front of the battery | -- | --
G102 | The left front side of the engine compartment on the left-front inner fender near the battery | Harness Routing Views | --
G103 | The right front side of the engine compartment on the right front side of the inner fender | Harness Routing Views | --
G104 | The center rear side of the engine on the intake manifold | Harness Routing Views | --
G105 (VIN 6) | The center rear of the engine, on the intake manifold | -- | --
G201 | Behind the left side of the kick panel | Harness Routing Views | --
G202 | The right side of the center IP behind the radio | Harness Routing Views | --
G203 | The junction-block case ground, under the left side of the IP | -- | --
G204 | Behind the right side of the kick panel | -- | --
G300 (4-Door) | Behind the trim panel of the right rear quarter | -- | --
G400 | The rear center of the luggage compartment | Harness Routing Views | --
G401 (2-Door) | The center of the liftgate, near the rear wiper motor | Harness Routing Views | --
G402 (2-Door) | The left side of the liftgate behind the trim panel | -- | --
P200 | the left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
P202 | The center of the engine compartment, on the bulkhead | Harness Routing Views | --
P203 | Behind the right kick panel | -- | --
P300 | Below the right rear passenger seat | Harness Routing Views | --
P400 | The left rear side of the luggage compartment | -- | --
P401 | The right rear of the luggage compartment | -- | --
P402 | The center rear side of the luggage compartment | Harness Routing Views | --
P403 (2-Door) | The upper right side of the liftgate | Harness Routing Views | --
P500 | The left front door | -- | --
P600 | The right front door | -- | --
S101 | The main harness, approximately 11 cm (4.5 in) from the breakout of the brake fluid level switch | Harness Routing Views | --
S111 (VIN 6) | The main harness, approximately 7 cm (2.8 in) from the ignition coil breakout | -- | --
S117 | The main harness, at the G103 breakout | Harness Routing Views | --
S122 | The main harness, at the relay box | Harness Routing Views | --
S126 | The engine harness, approximately 8 cm (3.1 in) from P202 | Harness Routing Views | --
S130 | The engine harness, approximately 5 cm (2 in) from the starter breakout | Harness Routing Views | --
S134 | The A/C jumper harness, approximately 15 cm (6 in) from the G103 breakout | -- | --
S151 | The main harness, approximately 5 cm (2 in) from the relay box | Harness Routing Views | --
S152 | The main harness, approximately 19 cm (7.4 in) from the C113 breakout | Harness Routing Views | --
S160 (VIN 2) | The engine Harness, approximately 20 cm (8 in) from P202 | -- | --
S161 (VIN 2) | The engine harness, approximately 4 cm (2 in) from the generator breakout | -- | --
S165 (VIN 2) | The engine harness, approximately 5 cm (2 in) from the starter breakout | Harness Routing Views | --
S167 | The engine harness, approximately 14 cm (6 in) from the C113 breakout | Harness Routing Views | --
S202 | The main harness, approximately 8 cm (3.125 in) from the breakout of the junction-block connector C6 | -- | --
S207 | The main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S208 (With ABS) | The main harness, approximately 12 (5 in) cm from the G201 breakout | -- | --
S209 | The main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S210 | The main harness, approximately 15 cm (6 in) from C208 | -- | --
S213 | The main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S215 (With ABS) | The main harness, approximately 4 cm (2 in) from the breakout of the junction-block connector C6 | -- | --
S222 | The IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC -OBD2) breakout | Harness Routing Views | --
S224 | The IP harness, approximately 5 cm (2 in) from the data link connector - (DLC -OBD2) breakout | Harness Routing Views | --
S235 | The IP harness, approximately 5 cm (2 in) from the C200 breakout | Harness Routing Views | --
S236 | The IP harness, approximately 8 cm (3.125 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views | --
S237 | The IP harness, approximately 10 cm (4 in) from the radio connector breakout | Harness Routing Views | --
S238 | The IP harness, approximately 3 cm (1.19 in) from the blower motor connector breakout | Harness Routing Views | --
S239 | The IP harness, approximately 11 cm (4.313 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views | --
S240 | The IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD 2) breakout | Harness Routing Views | --
S241 | The IP harness, approximately 5 cm (2 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views | --
S242 | The IP harness, at the breakout of the IP cluster assembly connector C3 | Harness Routing Views | --
S243 | The IP harness, approximately 5 cm (2 in) from the cigar-lighter connector breakout | Harness Routing Views | --
S244 | The main harness, approximately 23 cm (9.06 in) from P200 | -- | --
S245 | The IP harness, approximately 12 cm (5 in) from the breakout of the IP cluster assembly connector C3 | Harness Routing Views | --
S247 | The main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S254 | The IP harness, approximately 6 cm (2.375 in) from the C215 breakout | Harness Routing Views | --
S256 | The main harness, near the breakout of the junction-block connector C6 |  | --
S263 | The engine harness, approximately 3 cm (1.9 in) from the C205 breakout | Harness Routing Views | --
S301 (2-Door) | The floor harness, approximately 20 cm (8 in) from the center-console branch breakout | Harness Routing Views | --
S314 (4-Door With Power Door Locks) | The floor harness, approximately 25 cm (10 in) from the C201 breakout | Harness Routing Views | --
S315 | The fuel tank jumper harness, approximately 10 cm (4 in) from P300 | Harness Routing Views | --
S402 (2-Door) | The floor harness, approximately 5 cm (2 in) from the connector breakout of the left rear combination lamp | -- | --
S403 (2-Door) | The floor harness, approximately 5 cm (2 in) from the G400 breakout | -- | --
S406 (4-Door) | The floor harness, approximately 10 cm (4 in) from the connector breakout of the left rear combination lamp | -- | --
S407 (4-Door) | The floor harness, approximately 20 cm (8 in) from the connector breakout of the left rear combination lamp | -- | --
S408 (4-Door) | The floor harness, approximately 5 cm (2 in) from the C400 breakout | -- | --