Body Front End Adjustment Specifications. Chevrolet Metro 2000

For 1990-2009 cars

## Body Front End Adjustment Specifications 2 Door

#### 2-Door Model, Sheet Metal Tolerances

Location | Clearance Gap | Flushness
--- | --- | ---
Important: The following specifications are to be used to ensure the proper clearances and flushness of the front end body components after body repair procedures are complete.
1: Front Door to Fender | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
2: Hood to Air Inlet Grille | 6.0 mm (0.24 in) | --
3: Hood to Headlamp | 4.3 mm (0.17 in) | -2.0 to 0.0 mm (-0.08 to 0.00 in)
4: Hood to Fender | 3.6 mm (0.14 in) | -1.8 to 0.0 mm (-0.07 to 0.00 in)
5: Rocker Panel to Fender | 2.5 mm (0.10 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
6: Side Window to Windshield | 8.9 mm (0.35 in) | --

## Body Front End Adjustment Specifications 4 Door

#### 4-Door Model, Sheet Metal Tolerances

Location | Clearance Gap | Flushness
--- | --- | ---
Important: The following specifications are to be used to ensure the proper clearances and flushness of the front end body components after body repair procedures are complete.
1: Front Door to Fender | 5.0 mm (0.20 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
2: Hood to Air Inlet Grille | 6.0 mm (0.24 in) | --
3: Hood to Headlamp | 4.3 mm (0.17 in) | -2.0 to 0.0 mm (-0.08 to 0.00 in)
4: Hood to Fender | 3.6 mm (0.14 in) | -1.8 to 0.0 mm (-0.07 to 0.00 in)
5: Rocker Panel to Fender | 2.5 mm (0.10 in) | -1.0 to 0.0 mm (-0.04 to 0.00 in)
6: Side Window to Windshield | 8.9 mm (0.35 in) | --