Wheel Alignment Specifications. Chevrolet Metro 2000

For 1990-2009 cars

Operation | Service Allowed | Service Preferred
--- | --- | ---
Front

- Caster (non adjustable, for reference only)

+1.0° to +5.0°

+3.0°

- Cross Caster (non adjustable, for reference only)

0.0° to +0.75°

0.0°

- Camber

-0.5° to +1.5°

+0.5°

- Cross Camber

0.0° to +0.75°

0.0°

- Toe

0.0° to +0.16°

+0.08°

- Total Toe

0.0° to +0.32°

+0.16°

- Inside Turning Angle

--

38°

- Outside Turning Angle

--

32°

- Side Slip Limit

0 to 3 mm/m (0 to 0.118 in/1 in)

--

Rear

- Camber (non adjustable, for reference only)

-1.0° to +1.0°

0.0°

- Cross Camber (non adjustable, for reference only)

0.0° to +0.75°

0.0°

- Toe

+0.15° to +0.3°

+0.22°

- Total Toe

+0.3° to +0.6°

+0.45°

- Side Slip Limit

1 to 5 mm/m (0.197 to 0.39 in/1 in)

--