Braking Action Uneven - Front to Rear. Chevrolet Metro 2000

For 1990-2009 cars

Causes | Correction
--- | ---
Contaminated brake linings | Replace the brake linings.
Excessive vehicle loading | Refer to the tire placard for the vehicle capacity specification.
Leaking brake pipe or connection | Locate and repair the brake pipe or the connection.
Leaking caliper piston seal | Repair or replace the caliper.
Leaking master cylinder (internally) | Repair or replace the master cylinder.
Air in the brake system | Bleed the brake system.
Contaminated or improper brake fluid | Flush the brake system and repair the affected brake components.
Worn out brake linings | Replace the brake linings.
Uneven brake lining material | Replace the brake linings.
Glazed brake linings | Replace the brake linings.
Incorrect lining material | Replace the brake linings.
Linings damaged by abusive use | Replace the brake linings.
Scored rotor | Refinish the rotor surface or replace the rotor.
Loose front or rear brake assembly | Locate and tighten loose brake components.
Restricted brake fluid passage | Locate and repair the source of the brake fluid restriction.
Improperly adjusted parking brake | Adjust the parking brake.
Sticky caliper or caliper pistons | Repair or replace the caliper.
Improper rear brake adjustment | Adjust the rear brake linings.