Fastener Tightening Specifications. Chevrolet Metro 2000

For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Blower Case Bolts | 10 N·m | 89 lb in
Clutch Coil Wire Retainer Bolt | 2-2.5 N·m | 17.7-22.12 lb in
Compressor Bolts | 22.5-27.4 N·m | 16.5-20.1 lb ft
Compressor Bracket Front Bolts | 63.7-68.6 N·m | 46.8-50.4 lb ft
Compressor Bracket Right Bolt | 34.3-39.2 N·m | 25.2-28.8 lb ft
Compressor Discharge and Suction Hose Bolts | 9.8 N·m | 86.74 lb in
Compressor Pipe Fitting Bolt | 9.8 N·m | 86.74 lb in
Condenser Inlet Pipe Fitting Nut | 9.8 N·m | 86.74 lb in
Condenser Outlet Fitting Pipe Nut | 35 N·m | 26 lb ft
Discharge Hose to Condenser Nut | 9.8 N·m | 86.74 lb in
Heater Case Bolts and Nuts | 10 N·m | 89 lb in
Idler Pulley Locknut | 44.1-49.0 N·m | 32.4-36 lb ft
Pressure Plate Nut | 15-20 N·m | 10.8-15.2 lb ft
Pressure Relief Valve | 12-18 N·m | 106.2 lb in-13 lb ft
Receiver/Dryer-to-Evaporator Pipe Nut | 35 N·m | 26 lb ft