Wipers All Modes and Washer Inoperative. Chevrolet Metro 1999

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the system check? | -- | Go to Step 2 | Go to Wiper/Washer System Check

2

1. Turn the ignition switch to the ON position.
2. Backprobe the junction block connector C3 with a test lamp from cavity 7 to ground.

Does the test lamp light?

--

Go to Step 3

Go to Step 4

3 | Test for an open in the YEL/BLU wire between the junction block and the combination switch. Was an open found? | -- | Go to Step 6 | Go to Step 5
4 | Replace the junction block. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
5 | Replace the combination switch. Refer to Inflatable Restraint Steering Wheel Module Coil Replacement in Restraints. Is the repair complete? | -- | Go to Wiper/Washer System Check | --
6 | Repair the open. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Wiper/Washer System Check | --