HVAC Components. Chevrolet Metro 2000

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
A/C Compressor Clutch | The right side of the engine compartment, in front of the A/C compressor | -- | --
A/C Compressor Control Module | Below the right side of the IP, attached to the evaporator case | HVAC Component Views | HVAC Connector End Views
A/C Condenser Fan Motor | The right side of the grille, in front of the A/C condenser | HVAC Component Views | --
A/C Refrigerant (Dual) Pressure Switch | The right rear side of the engine compartment, near the strut tower | -- | --
A/C Switch | The center of the IP, above the radio | -- | HVAC Connector End Views
Blower Motor | Behind the right side of the IP | HVAC Component Views | HVAC Connector End Views
Blower Motor Resistor | Behind the right side of the IP, in the blower assembly | HVAC Component Views | HVAC Connector End Views
Blower Speed Selector Switch | The center of the IP, above the radio | HVAC Component Views | --
Fuse Box | The left side of the engine compartment, mounted on the left inner side of the fender, behind the relay box | Power and Grounding Component Views in wiring systems | Power and Grounding Connector End Views in wiring systems
Junction Block | Behind the left side of the IP | Power and Grounding Component Views in wiring systems | Power and Grounding Connector End Views in wiring systems
Relay Box | The left front engine compartment, near the battery | Power and Grounding Component Views in wiring systems | Power and Grounding Connector End Views in wiring systems
C111 (2 Cavities) (With A/C) | The main harness to the A/C jumper harness, on the right rear side of the engine compartment below the front wiper motor | Harness Routing Views in wiring systems | --
C112 (16 Cavities) | The main harness to the engine harness, on the right rear side of the engine compartment near the bulkhead | Harness Routing Views in wiring systems | Inline Harness Connector End Views in wiring systems
C113 (16 Cavities) | The main harness to the engine harness, on the right rear side of the engine compartment near the bulkhead | Harness Routing Views in wiring systems | Inline Harness Connector End Views in wiring systems
C200 (12 Cavities) | The main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in wiring systems | Inline Harness Connector End Views in wiring systems
C208 (8 Cavities) | The main harness to the IP harness, behind the left IP, near the junction block | Harness Routing Views in wiring systems | Inline Harness Connector End Views in wiring systems
C211 (6 Cavities) | The IP harness to the selector switch jumper for the blower speed , behind the center of the IP | Harness Routing Views in wiring systems | --
G102 | The left front side of the engine compartment on the left-front inner fender near the battery | Harness Routing Views in wiring systems | --
G103 | The right front side of the engine compartment on the right front side of the inner fender | Harness Routing Views in wiring systems | --
G201 | Behind the left side of the kick panel | Harness Routing Views in wiring systems | --
G202 | The right side of the center IP behind the radio | Harness Routing Views in wiring systems | --
P200 | The left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views in wiring systems | --
P202 | The center of the engine compartment, on the bulkhead | Harness Routing Views in wiring systems | --
S122 | The main harness, at the relay box | Harness Routing Views in wiring systems | --
S123 | The main harness, approximately 4 cm (2 in) from the connector breakout of the brake-fluid level switch | Harness Routing Views in wiring systems | --
S134 | The A/C jumper harness, approximately 15 cm (6 in) from the G103 breakout | -- | --
S202 | The main harness, approximately 8 cm (3.125 in) from the C6 breakout of the junction-block connector | -- | --
S207 | The main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S209 | The main harness, approximately 2 cm (1 in) from the G201 breakout | -- | --
S210 | The main harness, approximately 15 cm (6 in) from C208 | -- | --
S213 | The main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S232 | The IP harness, approximately 4 cm (2 in) from the C205 breakout | Harness Routing Views in wiring systems | --
S233 | The IP harness, approximately 8 cm (3.125 in) from the blower motor branch breakout | Harness Routing Views in wiring systems | --
S234 | The IP harness, approximately 1 cm (.375 in) from the diode-module connector breakout | Harness Routing Views in wiring systems | --
S238 | The IP harness, approximately 3 cm (1.19 in) from the blower-motor connector breakout | Harness Routing Views in wiring systems | --
S243 | The IP harness, approximately 5 cm (2 in) from the cigar-lighter connector breakout | Harness Routing Views in wiring systems | --
S247 | The main harness, approximately 18 cm (7.06 in) from P200 | -- | --
S254 | The IP harness, approximately 6 cm (2.375 in) from the C215 breakout | Harness Routing Views in wiring systems | --