Driver or Passenger Seat Back Cushion Cover Replacement. Chevrolet Metro 2000

For 1990-2009 cars

### Removal Procedure

1. Slide the seat assembly to the farthest rearward position.
2. Remove the inboard seat back hinge arm screw (2) from the seat assembly.
3. Position the seat back (1) forward.
4. Roll the cover (2) upward slowly and evenly.
5. Remove the cover (1) from the seat back (3).

### Installation Procedure

1. Roll the cover (1) down onto the seat back (3).
2. Install the inboard seat back hinge arm screw (2) to the seat assembly.
3. Return the seat back to the upright position.