Fasten Safety Belt Chime Inoperative. Chevrolet Metro 2000

For 1990-2009 cars

Step | Action | Value(s) | Yes | No
--- | --- | --- | --- | ---
1 | Did you perform the Audible Warnings System Check? | -- | Go to Step 2 | Go to Audible Warnings System Check
2 | With the seat belt unbuckled. Connect a test lamp from the seat belt switch connector cavity 2 to B+. Does the test lamp light? | -- | Go to Step 3 | Go to Step 4
3 | Test for continuity in the GRY/RED wire between connector cavity 2 of the seat belt switch and connector cavity 1 of the audio alarm module. Is there continuity in the GRY/RED wire? | 0-2ohms | Go to Step 8 | Go to Step 7
4 | Test for continuity in the BLK wire between the seat belt switch connector cavity 1 and G400. Is there continuity between cavity 1 and G400? | 0-2ohms | Go to Step 5 | Go to Step 6
5 | Replace the seat belt. Refer to Seat Belt Retractor Replacement - Left Front in Seat Belts Is the repair complete? | -- | Go to Audible Warnings System Check | --
6 | Repair the wire between connector cavity 1 of the seat belt switch and G400. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
7 | Repair the open GRY/RED wire between cavity 2 of the seat belt switch connector and cavity 1 of the audio alarm module connector. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | -- | Go to Audible Warnings System Check | --
8 | Replace the audio alarm module. Refer to Audio Alarm Module Replacement in Instrument Panel, Gauges and Console. Is the repair complete? | -- | Go to Audible Warnings System Check | --