Entertainment Components. Chevrolet Metro 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
LH Front Speaker | Left front door behind door trim panel | Entertainment Component Views | Entertainment Connector End Views
LH Rear Speaker (2-Door) | Left rear quarter trim panel | -- | Entertainment Connector End Views
(4-Door) | Rear window shelf, on the left side | Entertainment Component Views | Entertainment Connector End Views
Radio | Center of the IP | -- | Entertainment Connector End Views
RH Front Speaker | Right front door, behind the door trim panel | Entertainment Component Views | Entertainment Connector End Views
RH Rear Speaker (2-Door) | Right rear quarter trim panel | -- | Entertainment Connector End Views
(4-Door) | Rear window shelf, on right side | Entertainment Component Views | Entertainment Connector End Views
C203 (13 Cavities) | I/P harness to floor harness, behind left side of the IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C214 (2 Cavities) | I/P harness to left front speaker jumper harness, behind left kick panel | Harness Routing Views | --
C215 (2 Cavities) | I/P harness to the right front speaker jumper harness, behind the right kick panel | Harness Routing Views | --
C400 (10 Cavities) (4-Door) | Floor harness to luggage compartment harness, left front side of luggage compartment near the left rear speaker | Harness Routing Views | --
G202 | Right side of the center IP behind the radio | Harness Routing Views | --
P500 | Left front door | -- | --
P600 | Right front door | -- | --
S222 | IP harness, approximately 6 cm (2.375 in) from the data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S224 | IP harness, approximately 5 cm (2 in) from data link connector - (DLC-OBD2) breakout | Harness Routing Views | --
S237 | IP harness, approximately 10 cm (4 in) from the radio connector breakout | Harness Routing Views | --
S238 | IP harness, approximately 3 cm (1.19 in) from the blower motor connector breakout | Harness Routing Views | --
S243 | IP harness, approximately 5 cm (2 in) from the cigar lighter connector breakout | Harness Routing Views | --