Brake Caliper Bracket Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the brake pads. Refer to Brake Pad Inspection .
2. Remove 2 bolts and the caliper carrier from the vehicle.
3. Remove 2 caliper pins, with the boots, from the caliper carrier (1).

### Installation Procedure

1. Lubricate the caliper pins with silicone grease.
2. Install 2 caliper pins, with the boots, to the caliper carrier.

Notice: Use the correct fastener in the correct location. Replacement fasteners must be the correct part number for that application. Fasteners requiring replacement or fasteners requiring the use of thread locking compound or sealant are identified in the service procedure. Do not use paints, lubricants, or corrosion inhibitors on fasteners or fastener joint surfaces unless specified. These coatings affect fastener torque and joint clamping force and may damage the fastener. Use the correct tightening sequence and specifications when installing fasteners in order to avoid damage to parts and systems.

3. Install the caliper carrier (1) to the vehicle. Secure the carrier with 2 bolts.

Tighten
Tighten the caliper carrier bolts to 40-60 N·m (29-43 lb ft).

4. Install the linings. Refer to Brake Pad Inspection .