Passenger Car Zoning. Chevrolet Metro 2000

For 1990-2009 cars

All grounds, in-line connectors, pass-through grommets, and splices have identifying numbers that correspond to where they are located in the vehicle. The following table explains the numbering system.

#### Vehicle Zoning Table

Callout Numbers | Zone Description
--- | ---
100-199 | Engine compartment- All forward of the dash panel Note: 001-099 are additional for the engine compartment - ONLY to be used if all 100-199 items are used
200-299 | Within the instrument panel area
300-399 | Passenger compartment - From the instrument panel to the rear wheelhouse
400-499 | Luggage compartment - From the rear wheelhouse to the rear of the vehicle
500-599 | Within the left front door
600-699 | Within the right front door
700-799 | Within the left rear door
800-899 | Within the right rear door
900-999 | Within the luggage compartment lid or hatch