Fluid and Lubricant Recommendations. Chevrolet Metro 2001

For 1990-2009 cars

Application | Fluid/Lubricant
--- | ---
Automatic Transaxle | DEXRON®-III Automatic Transmission Fluid (GM P/N 12346143) or the equivalent
Chassis Lubrication | Chassis Lubricant (GM P/N 12377985), a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Clutch Linkage Pivot Points | Chassis Lubricant (GM P/N 12377985, a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Engine Coolant | A 50/50 mixture of clean water (preferably distilled) and a good quality Ethylene Glycol Base Coolant (GM P/N 1052753), an equivalent which conforms to GM Specification 1825M, or an approved recycled coolant which conforms to GM Specification 1825M. Refer to Explanation of Scheduled Services
Engine Oil | The engine oil with the American Petroleum Institute Certified For Gasoline Engines "Starburst" symbol of the correct viscosity. In order to determine the preferred viscosity for your vehicle's engine, refer to Explanation of Scheduled Services
Hood and Door Hinges | Multi-Purpose Lubricant, Superlube®, (GM P/N 12346241) or the equivalent.
Hood Latch Assembly and Secondary Latch | Lubriplate Lubricant Aerosol (GM P/N 12346293), a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB or the equivalent
Hydraulic Brake System | Delco Supreme 11® Brake Fluid (GM P/N 12377967), or an equivalent DOT-3 Brake Fluid.
Key Lock Cylinders | Multi-Purpose Lubricant, Superlube®, (GM P/N 12346241) or the equivalent
Manual Transaxle | GM Goodwrench Synthetic Manual Transmission Fluid (GM P/N 12346190) or an equivalent SAE 75W-90 GL-4 Gear Oil
Manual Transaxle Shift Linkage | Chassis Lubricant (GM P/N 12377985), a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB, or the equivalent
Parking Brake Cable Guides | Chassis Lubricant (GM P/N 12377985) or a lubricant meeting the requirements of NLGI # 2, Category LB or GC-LB
Power Steering System | DEXRON®-III Automatic Transmission Fluid (GM P/N 12346143) or the equivalent
Weatherstrip Conditioning | Dielectric Silicone Grease (GM P/N 12345579), Weatherstrip Lubricant-Krytox (GM P/N 3634770) or the equivalent.
Windshield Washer Solvent | GM Optikleen ® Washer Solvent (GM P/N 1051515) or the equivalent.