Wiper/Washer System Components. Chevrolet Metro 1998

For 1990-2009 cars

Name | Location | Locator View | Connector End View
--- | --- | --- | ---
Front Washer Pump | Left front side of the engine compartment, under the washer fluid reservoir | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Front Wiper Motor | Right rear side of the engine compartment, against the bulkhead | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Junction Block | Behind left side of the IP | Power and Grounding Component Views | Power and Grounding Connector End Views
Rear Washer Pump (2-Door LSi) | Left front side of the engine compartment under washer fluid reservoir | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Wiper Motor (2-Door LSi) | Center of the liftgate | Wiper/Washer Component Views | Wiper/Washer Connector End Views
Rear Wiper/Washer Switch (2-Door LSi) | In IP, left of the steering column | -- | Wiper/Washer Connector End Views
Turn Signal/Combination Switch | On steering column | -- | Lighting Systems Connector End Views
C200 (12 Cavities) | Main harness to the IP harness, behind the left IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C203 (13 Cavities) | I/P harness to floor harness, behind left side of the IP, near junction block | Harness Routing Views | Inline Harness Connector End Views
C402 (6 Cavities) (2-Door) | Floor harness to liftgate harness, right rear corner of vehicle | Harness Routing Views | --
G102 | Left front side of the engine compartment on the left front inner fender near battery | Harness Routing Views | --
G203 | Junction block case ground, under the left side of the IP | -- | --
G401 (2-Door) | Center of the liftgate, near rear wiper motor | Harness Routing Views | --
P200 | Left rear engine compartment, on the bulkhead, near the brake master cylinder | Harness Routing Views | --
P403 (2-Door) | Upper right side of the liftgate | Harness Routing Views | --
S115 | Main harness, approximately 35 cm (14 in) from the rear washer pump connector. | Harness Routing Views | --
S207 | Main harness, approximately 12 cm (5 in) from the G201 breakout | -- | --
S213 | Main harness, approximately 8 cm (3.125 in) from P200 | -- | --
S247 | Main harness, approximately 18 cm (7.06 in) from P200 | -- | --