Instrument Panel Cluster Trim Plate Bezel Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Remove the instrument cluster lower covers (7) by removing 2 screws.
2. Remove the following components from the steering column:

2.1. | 5 screws

2.2. | The upper steering column trim cover

2.3. | The lower steering column trim cover

3. Remove the instrument cluster bezel (8) by removing 4 screws.

### Installation Procedure

1. Install the instrument cluster bezel (8). Secure the trim panel with the 4 screws.
2. Install the upper and lower steering column trim covers. Secure the covers with the five screws.
3. Install the left and the right instrument cluster lower covers (7). Secure the covers with the 2 screws.