Dome Lamp Replacement. Chevrolet Metro 2001

For 1990-2009 cars

## Dome Lamp Replacement 2 Door

### Removal Procedure

1. Using a flat bladed tool, gently pry off the dome lamp lens (3).
2. Remove the 2 mounting screws (4) that retain the dome lamp .
3. Lower the dome lamp (2).
4. Disconnect the dome lamp electrical connector (1).
5. Remove the dome lamp (2) from the vehicle.

### Installation Procedure

1. Connect the dome lamp electrical connector (1).
2. Install the dome lamp (2) to the vehicle. Secure the lamp with the 2 screws (4).
3. Install the dome lamp lens (3) to the dome lamp (2).

## Dome Lamp Replacement 4 Door

### Removal Procedure

1. Using a flat-bladed tool, gently pry off the dome lamp lens (4).
2. Remove the 2 dome lamp nuts (3).
3. Lower the dome lamp (2).
4. Disconnect the dome lamp electrical connector (1).
5. Remove the dome lamp (2) from the vehicle.

### Installation Procedure

1. Connect the dome lamp electrical connector (1).
2. Install the dome lamp (2) to the vehicle. Secure the lamp with the 2 nuts (3).
3. Install the dome lamp lens (4) to the dome lamp (2).