Condenser Fan Always On. Chevrolet Metro 1999

For 1990-2009 cars

Step | Action | Yes | No
--- | --- | --- | ---
1 | Was the HVAC System Check performed? | Go to Step 2 | Go to HVAC System Check

2

1. Start the engine.
2. Turn the A/C off.

Does the air conditioning (A/C) compressor clutch engage?

Go to HVAC Compressor Clutch Does Not Disengage

Go to Step 3

3 | Remove the A/C 2 relay from the relay box. Does the A/C condenser fan motor stop? | Go to Step 4 | Go to Step 5
4 | Replace the A/C 2 relay. Refer to Condenser Fan Relay Replacement . Is the repair complete? | Go to HVAC System Check | --
5 | Repair the short to voltage between the A/C 2 relay and the A/C condenser fan motor in the BLU/BLK wire or in the RED/BLU wire. Refer to Wiring Repairs in Wiring Systems. Is the repair complete? | Go to HVAC System Check | --