Cupholder Replacement. Chevrolet Metro 1998

For 1990-2009 cars

### Removal Procedure

1. Remove the console from the vehicle. Refer to Console Replacement .
2. Remove the IP center trim bezel (4). Refer to Instrument Panel Center Trim Panel Replacement .
3. Remove the cup holder (8) from the instrument panel by removing 2 screws.

### Installation Procedure

1. Install the cup holder (8) to the instrument panel. Secure the cup holder with the 2 screws.
2. Install the IP center trim bezel (4) to the instrument panel. Refer to Instrument Panel Center Trim Panel Replacement .
3. Install the console to the vehicle. Refer to Console Replacement .