Rear Compartment Lid Lamp Lens and Bulb Replacement. Chevrolet Metro 1999

For 1990-2009 cars

### Removal Procedure

1. Open the rear compartment lid.
2. Turn the cargo lamp lens (6) counterclockwise in order to remove the lens from the cargo lamp.
3. Remove the cargo lamp bulb (3) from the lamp (2).
4. Pinch the retaining tab (4) in order to release the lamp (2) from the rear compartment shelf.
5. Disconnect the cargo lamp electrical connector (1).
6. Remove the lamp (2) from the vehicle.

### Installation Procedure

1. Connect the cargo lamp electrical connector (1).
2. Install the cargo lamp (2) to the rear compartment shelf. Ensure that the retaining tab (4) is completely engaged.
3. Install the cargo lamp bulb (3) to the lamp (2).
4. Install the cargo lamp lens (6) to the lamp by turning clockwise.
5. Close the rear compartment lid.