Horns Description. Chevrolet Metro 2000

For 1990-2009 cars

The horn (2) is under the hood. The horn (2) attaches to the left side of the upper tie bar. The horn sounds by depressing the horn buttons.

The horn buttons are on the edge of the steering wheel. The horn buttons are incorporated into the steering wheel pad. The horn buttons are not serviceable. If the horn buttons are inoperative, replace the inflatable restraint steering wheel module.